|  |  |
| --- | --- |
|  | **STANDARDS ASSOCIATION OF ZIMBABWE** |

DRAFT FOR  **PUBLIC COMMENT**

LATEST DATE FOR RECEIPT OF COMMENTS: **03-02-2025**

|  |
| --- |
| Our ref: BC 008/1 - D960-3/1  Draft Number BC 008/1 - D960-3/1  Date: **16-12-2024** |

TECHNICAL COMMITTEE BC 008/1: LPG

|  |
| --- |
| DRAFT ZIMBABWE STANDARD FOR  SPECIFICATION FOR THE HANDLING, STORAGE, DISTRIBUTION AND MAINTENANCE OF  LIQUEFIEDPETROLEUM GAS IN DOMESTIC, COMMERCIAL,  AND INDUSTRIAL INSTALLATIONS  PART 3: STORAGE AND FILLING PREMISES FOR REFILLABLE  LIQUEFIED PETROLEUM GAS (LPG) CONTAINERS OF GAS CAPACITY  NOT EXCEEDING 19 KG AND THE STORAGE OF INDIVIDUAL  GAS CONTAINERS NOT EXCEEDING 48 KG |

This draft is now available for **technical comment**. Your views and technical comments on it would be appreciated. If you have no specific comments to make but find it generally acceptable it would be helpful if you would notify us accordingly. Suggestions entailing revisions of the text should indicate the preferred wording using the attached template. The relevant clause number should be quoted against any comment.

All comments should be sent to the Committee Secretary **Mr P Chindara** at the address shown below.

Standards Association of Zimbabwe

P O Box 2259

Harare

E-mail: [pchindara@saz.org.zw](mailto:pchindara@saz.org.zw)

Website: [www.saz.org.zw](http://www.saz.org.zw)

THIS IS A DRAFT AND MUST NOT BE REGARDED OR USED AS A ZIMBABWE STANDARD.

|  |
| --- |
| **Copyrigh**t  Users of Zimbabwe National Standards are reminded that copyright subsists in all ZWS publications. No part of this publication may be produced in any form or by any means, electronic or mechanical, including photocopying or posting on the internet or an intranet, without permission in writing from the Director General of the Standards Association of Zimbabwe.  Orders for all national, international and foreign standards publications should be addressed to:  Director – Standards Development, Information and Training  Standards Association of Zimbabwe  P O Box 2259  Harare  Northridge Park  Borrowdale  Tel: 885511-2, 882017-9, 882021-2  Fax: 882020  **E-mail:**[***info@saz.org.zw***](mailto:info@saz.co.zw)  **Website:**[***www.saz.org.zw***](http://www.saz.org.zw) |

It is important that users of Zimbabwe Standards should ensure that they are in possession of the latest amendments or editions.

**AMENDMENTS**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **MD No.** | **Date of Issue** | **Text affected** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

Zimbabwe Standards are revised, when necessary, by issuing either amendments or revised editions. Suggestions for improvements will be welcome at all times.

**NOTICE**

The Standards Association of Zimbabwe is the registered owner of certification and registration marks shown in Information Services Publication No. 2, one of which is shown below. The presence of a certification mark on a product is an independent assurance that the product complies with the requirements of the relevant Zimbabwe Standard.



A certification mark may be used by the manufacturers only under licence from the Association. Particulars of the conditions under which licences are granted may be obtained from:

Director General

Standards Association of Zimbabwe

P O Box 2259

Harare

Northridge Park

Borrowdale

Telephone: 885511-2/882017-9/882021

Fax: 882020

E-mail: info@saz.org.zw

Website: [www.saz.org.zw](http://www.saz.org.zw)

**Contents** Page

Foreword 2

1. Scope 5

2. Definitions 5

3. Properties of LPG and Precautions to be Observed 7

4. Location, Design and Control of Filling Premises

With or Without A Storage Area 8

5. Filling Equipment 12

6. Containers 13

7. Operators 13

8. Inspection Procedure 14

9. Filling Procedure 17

10. Handling and Storage of LPG Containers 18

11. Prevention and Control of Fires Involving LPG 24

12. Model LPG Filling Area…………………………………………… 37

**Foreword**

This draft Zimbabwe Standard ZWS 960: The handling, storage, distribution and maintenance of liquefied petroleum gas in domestic, commercial, and industrial installations: Part 3:: Storage and filling premises for refillable liquefied petroleum gas (LPG) containers of gas capacity not exceeding 19 kg and the storage of individual gas containers not exceeding 48 kg, is based on SANS 10087-7

This standard was prepared by technical committee BC 008: LPG, under the general direction of the Building and Civil Engineering Sector .

First Published ,2012 as ZWS 960 Part 3

First revision, 2024 as ZWS 960 Part 3

ZWS 960 consists of the following parts, under the general title, The handling, storage,

distribution and maintenance of liquefied petroleum gas in domestic, commercial, and industrial

installations:

Part 1 : Liquefied petroleum gas installations involving gas storage containers of

individual water capacity not exceeding 500 ℓ and a combined water capacity not exceeding 3 000 ℓ per installation.

Part 2 : Liquefied petroleum gas installations involving storage vessels of individual

water capacity exceeding 500 ℓ.

Part 3 : Storage and filling premises for refillable liquefied petroleum gas (LPG)

containers of gas capacity not exceeding 19 kg and the storage of individual gas containers not exceeding 48 kg.

This Zimbabwe Standard makes reference to the following standards:

EN 671 : Fixed fire fighting systems – Hose systems

Part 1 : Hose reels with semi-rigid hose.

SANS 543 : Fire hose reels (with semi-rigid hose).

SANS 1186 : Symbolic safety signs

Part 1 : Standard signs and general requirements.

SANS 1825 : Gas cylinder test stations – General requirements for periodic inspection

and testing of portable and transportable refillable gas pressure receptacles.

SANS 1910 : Portable refillable fire extinguishers.

SANS 10019 : Transportable containers for compressed, dissolved and liquefied gases –

Basic design, manufacture, use and maintenance.

SANS 10086 : The installation, inspection and maintenance of equipment used in

Explosive atmospheres.

Part 1 : Installations including surface installations on mines.

SANS 10105 : The use and control of fire-fighting equipment

Part 1 : Portable and wheeled(mobile) fire extinguishers.

Part 2 : Fire hose reels and above ground hydrants.

SANS 10108 : The classification of hazardous locations and the selection of apparatus

for use in such locations.

ZWS 960 : The handling, storage, distribution and maintenance of liquefied petroleum gas in domestic, commercial, and industrial installations.

Part 1 : Liquefied petroleum gas installations involving gas storage containers of individual water capacity not exceeding 500 ℓ and a combined water capacity not exceeding 3 000 ℓ per installation.

Part 2 : Liquefied petroleum gas installations involving storage vessels of individual water capacity exceeding 500 ℓ.

ZWS 965 : Liquefied petroleum gas.

Zimbabwe Model Building By-laws.

ZIMBABWE STANDARD SPECIFICATION

FOR

THE HANDLING, STORAGE, DISTRIBUTION AND MAINTENANCE OF

LIQUEFIEDPETROLEUM GAS IN DOMESTIC, COMMERCIAL,

AND INDUSTRIAL INSTALLATIONS

PART 3: STORAGE AND FILLING PREMISES FOR REFILLABLE

LIQUEFIED PETROLEUM GAS (LPG) CONTAINERS OF GAS CAPACITY

NOT EXCEEDING 19 KG AND THE STORAGE OF INDIVIDUAL

GAS CONTAINERS NOT EXCEEDING 48 KG

(First revision ZWS 960 Part 3:2012)

1. **Scope**

This part of ZWS 960 specifies the minimum requirements for the location and installation of, and operations at, filling premises for the filling of liquefied petroleum gas (LPG) containers of gas capacity not exceeding 19 kg, including the storage of individual gas containers not exceeding 48 kg. It identifies safe methods of filling and storing refillable containers and makes recommendations towards safe working procedures that cover all aspects of the storage of containers.

This part of ZWS 960 also covers the storage of non-refillable containers.

**Note.** The titles of the publications referred to in this standard are listed in the Preface.